<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.28.0-Firenze">
  <identifier>FGDS.SB_SUBDIST_POLY</identifier>
  <parentidentifier></parentidentifier>
  <language>THA</language>
  <type>dataset</type>
  <title>FGDS.SB_SUBDIST_POLY</title>
  <abstract>REQUIRED: A brief narrative summary of the data set.

REQUIRED: A summary of the intentions with which the data set was developed.</abstract>
  <keywords vocabulary="gmd:topicCategory">
    <keyword>REQUIRED: Common-use word or phrase used to describe the subject of the data set.</keyword>
  </keywords>
  <links>
    <link url="file://\\PCBMA99\H$\updistrict52\subdist" name="ArcInfo Coverage" mimeType="" size="" description="" format="" type="Local Area Network"/>
  </links>
  <fees></fees>
  <constraints type="Access">REQUIRED: Restrictions and legal prerequisites for accessing the data set.</constraints>
  <rights>REQUIRED: Restrictions and legal prerequisites for using the data set after access is granted.</rights>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["WGS 84 / UTM zone 47N",BASEGEOGCRS["WGS 84",ENSEMBLE["World Geodetic System 1984 ensemble",MEMBER["World Geodetic System 1984 (Transit)"],MEMBER["World Geodetic System 1984 (G730)"],MEMBER["World Geodetic System 1984 (G873)"],MEMBER["World Geodetic System 1984 (G1150)"],MEMBER["World Geodetic System 1984 (G1674)"],MEMBER["World Geodetic System 1984 (G1762)"],MEMBER["World Geodetic System 1984 (G2139)"],ELLIPSOID["WGS 84",6378137,298.257223563,LENGTHUNIT["metre",1]],ENSEMBLEACCURACY[2.0]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4326]],CONVERSION["UTM zone 47N",METHOD["Transverse Mercator",ID["EPSG",9807]],PARAMETER["Latitude of natural origin",0,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8801]],PARAMETER["Longitude of natural origin",99,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8802]],PARAMETER["Scale factor at natural origin",0.9996,SCALEUNIT["unity",1],ID["EPSG",8805]],PARAMETER["False easting",500000,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",0,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["(E)",east,ORDER[1],LENGTHUNIT["metre",1]],AXIS["(N)",north,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Engineering survey, topographic mapping."],AREA["Between 96°E and 102°E, northern hemisphere between equator and 84°N, onshore and offshore. China. Indonesia. Laos. Malaysia - West Malaysia. Mongolia. Myanmar (Burma). Russian Federation. Thailand."],BBOX[0,96,84,102]],ID["EPSG",32647]]</wkt>
      <proj4>+proj=utm +zone=47 +datum=WGS84 +units=m +no_defs</proj4>
      <srsid>3131</srsid>
      <srid>32647</srid>
      <authid>EPSG:32647</authid>
      <description>WGS 84 / UTM zone 47N</description>
      <projectionacronym>utm</projectionacronym>
      <ellipsoidacronym>EPSG:7030</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial maxz="0" crs="EPSG:32647" minx="637000" dimensions="2" miny="1491881.5" maxx="709876" minz="0" maxy="1547000"/>
  </extent>
</qgis>
